{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":63,"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":77,"n_cols":10,"rows_kept":77,"merged":[[0,0,0,9],[1,0,1,9],[2,0,2,9],[76,0,76,6],[77,0,77,9],[78,0,78,6],[78,7,78,9],[79,0,79,6],[79,7,79,9]],"flags":["formulas_cached_only"]}
["  厨房设备报价清单  "]
["2018-09-05"]
["需方单位：福建省轻纺（控股）有限责任公司职工食堂               联系人：刘炜晶                 电话：0591-87510901           "]
["序号","设备名称","规格型号","数量","单位","单 价","金 额","品牌","技术参数","参考图片"]
["A","热厨间"]
["A1","调料拼台","300*1100*800+400",3,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                       \n2.δ1.0mm不锈钢侧板。                                                                                                                                                                                                                                                                                                               "]
["A2","电磁双炒单尾炉","1800*1100*800+400",1,"台",null,null,"摩力斯","1.全优质不锈钢结构设计，更加坚固耐用。\n2.采用技术领先的德国Infeneon IGBT。\n3.升温快，热效率高达92%，提高出菜率，节省50%以上。\n4.全新防水、防油烟、防虫设计。5.自动安全保护功能，性能更加可靠。6.三重立体防辐射外壳屏蔽设计。\n7.智能磁控开关控制，液晶显示一目了然。\n8.电量：15KW*2/380V"]
["A3","电磁一小炒一大煮炉","1900*1100*800+400",1,"台",null,null,"摩力斯","1.全优质不锈钢结构设计，更加坚固耐用。\n2.采用技术领先的德国Infeneon IGBT。\n3.升温快，热效率高达92%，提高出菜率，节省50%以上。\n4.全新防水、防油烟、防虫设计。5.自动安全保护功能，性能更加可靠。6.三重立体防辐射外壳屏蔽设计。\n7.智能磁控开关控制，液晶显示一目了然。\n8.电量：15KW+20KW/380V"]
["A4","电磁四眼煲仔炉","800*800*800+150",1,"台",null,null,"摩力斯","1.全优质不锈钢结构设计，更加坚固耐用。\n2.采用技术领先的德国Infeneon IGBT。\n3.升温快，热效率高达92%，提高出菜率，节省50%以上。\n4.全新防水、防油烟、防虫设计。5.自动安全保护功能，性能更加可靠。6.三重立体防辐射外壳屏蔽设计。\n7.智能磁控开关控制，液晶显示一目了然。\n8.电量：3.5KW*4/380V"]
["A5","电磁单头矮汤炉","650*750*500+600",1,"台",null,null,"摩力斯","1.全优质不锈钢结构设计，更加坚固耐用。\n2.采用技术领先的德国Infeneon IGBT。\n3.升温快，热效率高达92%，提高出菜率，节省50%以上。\n4.全新防水、防油烟、防虫设计。5.自动安全保护功能，性能更加可靠。6.三重立体防辐射外壳屏蔽设计。\n7.智能磁控开关控制，液晶显示一目了然。\n8.电量：15KW/380V"]
["A6","电磁三门海鲜蒸柜","1000*900*1850",1,"台",null,null,"摩力斯","1.全优质不锈钢结构设计，更加坚固耐用。\n2.采用技术领先的德国Infeneon IGBT。\n3.升温快，热效率高达92%，提高出菜率，节省50%以上。\n4.全新防水、防油烟、防虫设计。5.自动安全保护功能，性能更加可靠。6.三重立体防辐射外壳屏蔽设计。\n7.智能磁控开关控制，液晶显示一目了然。\n8.电量：20KW/380V"]
["A7","电双门蒸饭车","24盘",1,"台",null,null,"睿弘   美厨","1.采用优质不锈钢磨砂板，δ1.2mm不锈钢面板，加垫发泡隔热层。2.加强梁国标3.5mm*40mm*40mm 角铁焊接组成，所有角铁架涂有酚醇防锈漆。3.全自动进水，全自动动力系统。4.液压拉伸成形饭盘。5.一旦缺水自动断电，自动防止干烧，充分解决发热管干烧现象。6.电量：12KW*2/380V，蒸饭时间约45分钟。"]
["A9","双通工作台","1800*800*800",3,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板、底夹15mm高密度板及防潮镀锌板。     \n2.柜内活动层板δ1.0mm不锈钢板。  　                                                                                                                 \n3.δ1.0mm不锈钢支撑架。                                                                                                                               \n4.推拉门δ0.8mm不锈钢板 。       　　　　　　　　　　　　　　　　　\n5.台通脚δ1.2mm不锈钢ф51mm重力脚。    　　　　　　　　　　　　　　　　　"]
["A10","双层工作台","1500*800*800",2,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板、底夹15mm高密度板。                                                                                                                2.底层板δ1.0mm不锈钢,横梁δ1.0mm不锈钢方管。                                                                                                                          \n3.δ1.0mm不锈钢支撑架。         \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。                                                                                                                "]
["A11","保鲜工作台","1800*750*800",3,"台",null,null,"雅绅宝","1.温度范围：+5℃～-5℃，智能电子温控。                                                                       　　　　　　　　　　   　\n2.制冷剂：环保无氟制冷剂，环保发泡保温材料。               \n3.制冷形式：直冷。  \n4.电量：0.5KW/220V                                                                                                                   "]
["A12","开水器连底座","6KW",1,"台",null,null,"荣麦","1.工作过程全自动化，使用方便。\n2.采用全包围技术结构及聚氨脂发泡保温，保温效果良好。\n3.本机设有缺水、断电装置，有效保护电热管。\n4.容量：60L。\n5.电量：6KW/380V"]
["A13","单星水池","700*700*950",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                                                                                                                         \n2.δ1.0mm不锈钢侧板，机冲星盆尺寸：500*500*300（深）。                                                                                             \n3.δ1.0mm不锈钢支撑架。                                                                                                                                            \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。"]
["A14","双温六门冷柜","1810*730*1945",2,"台",null,null,"雅绅宝","1.温度范围：+5℃～-5℃/+0℃～-12℃，智能电子温控。                                                                       　　　　　　　　　　   　\n2.制冷剂：环保无氟制冷剂，环保发泡保温材料。               \n3.制冷形式：直冷。  \n4.电量：0.5KW/220V                                                                                                                   "]
["B","粗加工间",{"$nulls":4},0]
["B1","三星水池","1800*700*950",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                                                                                                                         \n2.δ1.0mm不锈钢侧板，机冲星盆尺寸：500*500*300（深）。                                                                                             \n3.δ1.0mm不锈钢支撑架。                                                                                                                                            \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。"]
["B2","大单星水池","1000*700*950",2,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                                                                                                                         \n2.δ1.0mm不锈钢侧板，机冲星盆尺寸：800*500*300（深）。                                                                                             \n3.δ1.0mm不锈钢支撑架。                                                                                                                                            \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。"]
["B3","双层工作台","1500*700*800",2,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板、底夹15mm高密度板。                                                                                                                2.底层板δ1.0mm不锈钢,横梁δ1.0mm不锈钢方管。                                                                                                                          \n3.δ1.0mm不锈钢支撑架。         \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。                                                                                                                "]
["B4","格栅四层存放架","1500*500*1500",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。\n2.δ1.0mm不锈钢支撑架。"]
["B5","格栅四层存放架","1200*500*1500",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。\n2.δ1.0mm不锈钢支撑架。"]
["C","仓库",{"$nulls":4},0]
["C1","板式四层存放架","1200*500*1500",3,"台",null,0,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。\n2.δ1.0mm不锈钢支撑架。"]
["C2","格栅米面架","1500*500*300",2,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。\n2.δ1.0mm不锈钢支撑架。"]
["C3","板式四层存放架","1500*500*1500",2,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。\n2.δ1.0mm不锈钢支撑架。"]
["D","洗碗间",{"$nulls":4},0]
["D1","收污台","1800*700*950",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                                                                                                                                        2.δ1.0mm不锈钢支撑架。          \n3.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。                                                                                                                                                                                                              "]
["D2","大单星水池","1000*700*950",2,"台",null,0,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                                                                                                                         \n2.δ1.0mm不锈钢侧板，机冲星盆尺寸：800*500*300（深）。                                                                                             \n3.δ1.0mm不锈钢支撑架。                                                                                                                                            \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。"]
["D3","三星水池","1800*700*950",1,"台",null,0,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                                                                                                                         \n2.δ1.0mm不锈钢侧板，机冲星盆尺寸：500*500*300（深）。                                                                                             \n3.δ1.0mm不锈钢支撑架。                                                                                                                                            \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。"]
["D4","格栅四层存放架","1500*500*1500",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。\n2.δ1.0mm不锈钢支撑架。"]
["D5","热风循环发泡双门消毒柜","1310*650*1980",1,"台",null,null,"睿弘   美厨","1、双层全不锈钢，聚氨脂发泡，厚度δ1.0mm。\n2、热风循环消毒温度：+20℃～+100℃，智能电子温控。\n3、热风循环无死角，杀菌更彻底。\n4、配不锈钢活动消毒筐。\n5、电量：4.4KW/220V"]
["D6","四门储碗柜","1100*500*1800",2,"台",null,null,"厂制品","1.采用优质不锈钢磨砂板 ,柜外壳δ1.2mm不锈钢面板。                                                                                                                                   2.柜内活动层板δ1.0mm不锈钢板。                 　　　　　　　　　　　                                                                            　\n3.δ1.0mm不锈钢支撑架。 \n4.推拉门δ1.0mm不锈钢板。                                                                                                                             \n5.台通脚δ1.2mm不锈钢ф51mm重力脚。         　　　　　　　　　　　                                                                            　"]
["D7","开水器连底座","6KW",1,"台",null,null,"荣麦","1.工作过程全自动化，使用方便。\n2.采用全包围技术结构及聚氨脂发泡保温，保温效果良好。\n3.本机设有缺水、断电装置，有效保护电热管。\n4.容量：60L。\n5.电量：6KW/380V"]
["E","自助打菜区",{"$nulls":4},0]
["E1","带柜门五格保温售卖台","1800*700*800",3,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                                                                                                                       \n2.可放GN不锈钢份数盘。                                                                                                                \n3.电量：2KW/220V，自动恒温控制。  \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。                                                                                                                "]
["E2","炖品保温台","1500*700*800",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。                                                                                                                      \n2.冲孔保温台面。                                                                                                                \n3.电量：2KW/220V，自动恒温控制。  \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。                                                                                                                "]
["E3","保温饭台","600*700*800",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。\n2.车盖采用δ1.0mm不锈钢板。\n3.不锈钢排铰连接；两边对开揿门。\n4.配4只3寸防滑、耐磨万向轮优质胶轮，2只带刹车製。"]
["E4","保温汤台","600*700*800",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板。\n2.车盖采用δ1.0mm不锈钢板。\n3.不锈钢排铰连接；两边对开揿门。\n4.配4只3寸防滑、耐磨万向轮优质胶轮，2只带刹车製。"]
["E5","不锈钢滑台","7000*350",2,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.5mm不锈钢面板。                                                                                                                \n2.δ1.0mm不锈钢侧板。"]
["E6","光波双门消毒柜","1210*560*1880",1,"台",null,null,"明盛","1、双层全不锈钢，聚氨脂发泡，厚度δ1.0mm。\n2、热风循环消毒温度：+20℃～+100℃，智能电子温控。\n3、热风循环无死角，杀菌更彻底。\n4、配不锈钢活动消毒筐。\n5、电量：4.4KW/220V"]
["E7","双层工作台","1500*700*800",1,"台",null,null,"厂制品","1.采用优质304不锈钢磨砂板，δ1.2mm不锈钢面板、底夹15mm高密度板。                                                                                                                2.底层板δ1.0mm不锈钢,横梁δ1.0mm不锈钢方管。                                                                                                                          \n3.δ1.0mm不锈钢支撑架。         \n4.台通脚δ1.2mm不锈钢圆管ф38mm及包钢调节脚组成。                                                                                                                "]
[null,"厨房排烟系统",{"$nulls":4},0]
[2,"主厨间不锈钢一体烟罩","LX1200X500",9.7,"米",null,null,"厂制品","优质不锈钢磨砂板厚1.2mm"]
[3,"不锈钢烟罩隔油网","500X500",18,"片",null,null,"厂制品","优质不锈钢磨砂板厚1.0mm，格网覆边成瓦楞状。"]
[4,"防爆灯",null,7,"个",null,null,"厂制品","专用照明灯，防潮、防腐蚀、防油"]
[5,"不锈钢炉灶后封板",null,9,"米",null,null,"厂制品","优质不锈钢磨砂板厚1.0mm"]
[6,"镀锌油烟管","700X500",25,"米",null,null,"厂制品","优质镀锌板厚1.0mm"]
[7,"镀锌主烟管","700X500",10,"米",null,null,"厂制品","优质镀锌板厚1.0mm"]
[8,"镀锌烟管三通",null,3,"个",null,null,"厂制品","优质镀锌板厚1.0mm"]
[9,"镀锌烟管弯头",null,5,"个",null,null,"厂制品","优质镀锌板厚1.0mm"]
[10,"镀锌烟管S弯",null,2,"个",null,null,"厂制品","优质镀锌板厚1.0mm"]
[11,"吊杆及固定码",null,1,"套",null,null,"厂制品","镀锌全螺纹牙丝杆，角铁3#"]
[12,"法兰及四边扣",null,1,"项",null,null,"厂制品","角铁3#"]
[13,"排烟风机","11KW",1,"台",null,null,"国通","机身结构紧凑，风量大、效率高，适用于厨房抽油烟的通风换气"]
[14,"风机支架及防震垫",null,1,"套",null,null,"厂制品","采用10#槽钢，2度油漆，防锈处理，配减震垫"]
[15,"风机变径接口",null,2,"个",null,null,"厂制品","优质镀锌板厚1.0mm"]
[16,"风机软接",null,1,"个",null,null,"厂制品","高强度PVC涂塑布"]
[17,"风机控制箱","60A",1,"台",null,null,"上海","选用适配功率电控箱，弱电控制、缺相、过载、相序错均跳闸，安全配置。"]
[18,"低空油烟净化器","26000风量",1,"台",null,null,"宇风","采用静电+机械的双重净化结构，有效去除油烟粒子，达到净化效果"]
[19,"净化器支架",null,1,"套",null,null,"厂制品","采用10#槽钢，2度油漆，防锈处理"]
[20,"净化器变径接口",null,2,"个",null,null,"厂制品","优质镀锌板厚1.0mm"]
[21,"接油盘",null,1,"个",null,null,"厂制品","优质镀锌板厚1.0mm"]
[22,"油杯",null,5,"个",null,null,"厂制品","优质不锈钢磨砂板厚1.0mm"]
[23,"排烟管道防漏专用胶",null,1,"项",null,null,"厂制品","国标"]
[null,"厨房鲜风系统",{"$nulls":4},0]
[1,"不锈钢六角鲜风管","500*320",18,"米",null,null,"厂制品","优质不锈钢磨砂板厚1.0mm"]
[2,"不锈钢鲜风管弯头","500*320",3,"个",null,null,"厂制品","优质不锈钢磨砂板厚1.0mm"]
[3,"吊杆及固定码",null,6,"套",null,null,"厂制品","镀锌全螺纹牙丝杆，角铁3#"]
[4,"法兰及四边扣",null,3,"对",null,null,"厂制品","角铁3#"]
[5,"铝合金鲜风咀",null,18,"个",null,null,"厂制品","可人工调节方向"]
[6,"水冷鲜风机","7500风量",1,"台",null,null,"普泽","1.全新风送入，岗位降温。特种纸制蜂窝结构材料，降温效率达80%以上。\n2.室内吊挂式，外墙仅见百叶风口，美观高档。\n3.自动间歇加注自来水方式。\n4.电量：0.55KW/220V"]
[7,"鲜风机支架",null,1,"套",null,null,"厂制品","角铁4#"]
[8,"鲜风管变径接口",null,1,"个",null,null,"厂制品","优质不锈钢磨砂板厚1.0mm"]
[{"$nulls":7},"总价"]